# Uses of Package
util

- Packages that use util
  Package | Description
  --- | ---
  broadcast | This package contains classes implementing the generation and synchronized dispatch of SiGML sequences over UDP to accompany a broadcast TV transmission.
  hnscnvt | This package implements the processing of HamNoSys 4 sign data in various input formats to give the corresponding HamNoSysML (HML) and gestural SiGML representations.
  sigmlinlib | This package defines the classes that define the main SiGML Input Library API, including the provision of a networked SiGML signing data input service using TCP/IP and UDP server sockets, suitable for use by an avatar based SiGML animation module.
  util | A collection of utility classes for the SiGML Input Library.

- Classes in util used by broadcast
  Class and Description
  Logging Interface defining a very simple file-based logging system.

- Classes in util used by hnscnvt
  Class and Description
  HamNameMap Provides mapping in both directions between HamNoSys token names and the corresponding octet values (classic HNS 3 character values), based on data from a Properties file.

- Classes in util used by sigmlinlib
  Class and Description
  Logging Interface defining a very simple file-based logging system.

- Classes in util used by util
  Class and Description
  AsciiIdMapper This class supports the mapping of ISO-8859-1/CP-1252 identifiers to ASCII-compatible form based on a mapping table file for individual characters.
  HamNameMap Provides mapping in both directions between HamNoSys token names and the corresponding octet values (classic HNS 3 character values), based on data from a Properties file.
  HNSOctetUCSMap Defines mappings in both directions between HNS 8-bit character code values (octets) and HamNoSys-UCS characters, most of which are in the UCS private use area.
  Logging Interface defining a very simple file-based logging system.
  RE.AV A structure that records the result of a scan for an attribute='value' string.